Hello,

On first, install the driver: "UsbDriver_SL500"
Wait 30 seconds and plug the card reader.
Wait for see final installation of driver.

And on each DATEC:
==> If JPB cards:
Go on the menu "CARDS MANAGMENT"
Change shooting range number for: your number
and change code for: your code
==> If Promatic cards:
Place the manager card on DATEC to automaic initialise.

Important:
---------
For the USB reader, the first time you use,
 Put a manager card on reader to initialise the security.
 If that not working, delete or rename file codes.txt then reload software and present manager card.


How use on Normal mode:
----------------------
Put a card on reader; You must see screen change.
On right screen you see how many clays is on this card.
Change the value
If you want, change the first line of text zone (Printed on TV screen)
then click to save button.


How use to change function of your card:
---------------------------------------
Put a card on reader; You must see screen change.
Select menu: "Change type of card"
select menu: "command for change memory position"
Now the function of your card are modified.


How use to make an automatic selection of course type for JPB cards:
-----------------------------------------------------
On the screen, you have 3 zones for change:
On down the text mode where you write even you want
On up right: "Counter 1 to 3" : enter a number (not important when you use promatic tokens)
On "Memory Position" : You must enter the number you want use.

Example:
1         Olympic trench
2         Universal trench
7         DTL
15        COMPACK N° 1
25        COMPACK N° 15

When you present this card on datec mifare reader, if you datec are not on lauching sequence, 
the datec change memory position for your choice without password or master card.

Good use.
JPB



